Pset_AirSideSystemInformation

BACnet MVD

#### 6.2.4.1 Pset_AirSideSystemInformation

PSET_TYPEDRIVENOVERRIDE / IfcSpace,IfcZone,IfcSpatialZone

Natural language names

| Air Side System Information

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Name

P_SINGLEVALUE / IfcLabel

| Name | The name of the air side system.
| 名前 | 空調方式の名称。

Description

P_SINGLEVALUE / IfcLabel

| Description | The description of the air side system.
| 説明 | 空調方式の説明。

AirSideSystemType

P_ENUMERATEDVALUE / IfcLabel / PEnum_AirSideSystemType

| Air Side System Type | This enumeration specifies the basic types of possible air side systems (e.g., Constant Volume, Variable Volume, etc.).

AirSideSystemDistributionType

P_ENUMERATEDVALUE / IfcLabel / PEnum_AirSideSystemDistributionType

| Air Side System Distribution Type | This enumeration defines the basic types of air side systems (e.g., SingleDuct, DualDuct, Multizone, etc.).
| 搬送方式 | 基本的な空調方式（単一ダクト、二重ダクト、マルチゾーン等）。

TotalAirflow

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Total Airflow | The total design supply air flowrate required for the system for either heating or cooling conditions, whichever is greater.
| 給気量 | 暖房、冷房の条件の、いずれか大きい条件で要求される設計給気量。

EnergyGainTotal

P_SINGLEVALUE / IfcPowerMeasure

| Energy Gain Total | The total amount of energy gains for the spaces served by the system during the peak cooling conditions, plus any system-level total energy gains.
| 総熱取得 | 居室の最大冷房負荷と空調システム（機器等）の再熱負荷による最大熱負荷。

AirflowSensible

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Airflow Sensible | The air flowrate required to satisfy the sensible peak loads.
| 顕熱空調給気量 | 最大潜熱負荷に対応する給気量。

EnergyGainSensible

P_SINGLEVALUE / IfcPowerMeasure

| Energy Gain Sensible | The sum of total energy gains for the spaces served by the system during the peak cooling conditions, plus any system-level sensible energy gains.
| 顕熱空調負荷 | ピーク時各居室の最大冷房負荷と空調システムの顕熱負荷による最大顕熱負荷。

EnergyLoss

P_SINGLEVALUE / IfcPowerMeasure

| Energy Loss | The sum of energy losses for the spaces served by the system during the peak heating conditions.
| 熱（エネルギー）ロス | ピーク時空調システム最大暖房負荷を提供する際の熱ロス。

LightingDiversity

P_SINGLEVALUE / IfcPositiveRatioMeasure *

| Lighting Diversity | Lighting diversity.
| 照明負荷係数 | 照明負荷係数。

InfiltrationDiversitySummer

P_SINGLEVALUE / IfcPositiveRatioMeasure *

| Infiltration Diversity Summer | Diversity factor for Summer infiltration.
| 夏期すき間換気率 | 夏期すき間換気率。

InfiltrationDiversityWinter

P_SINGLEVALUE / IfcPositiveRatioMeasure *

| Infiltration Diversity Winter | Diversity factor for Winter infiltration.
| 冬期すき間換気率 | 冬期すき間換気率。

ApplianceDiversity

P_SINGLEVALUE / IfcPositiveRatioMeasure *

| Appliance Diversity | Diversity of appliance load.
| 機器の負荷率 | 機器の負荷率。

LoadSafetyFactor

P_SINGLEVALUE / IfcPositiveRatioMeasure *

| Load Safety Factor | Load safety factor.
| 負荷の安全率 | 空調負荷計算用の安全率（割増係数）。

HeatingTemperatureDelta

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Heating Temperature Delta | Heating temperature difference for calculating space air flow rates.
| 暖房時送風温度差 | 空調送風量計算用の暖房給気温度差。

CoolingTemperatureDelta

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Cooling Temperature Delta | Cooling temperature difference for calculating space air flow rates.
| 冷房時送風温度差 | 空調送風量計算用の冷房給気温度差。

Ventilation

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Ventilation | Required outside air ventilation.
| 外気量 | 要求された外気量。

FanPower

P_SINGLEVALUE / IfcPowerMeasure

| Fan Power | Fan motor loads contributing to the cooling load.
| 送風機電力消費量 | 送風機モーターからの熱取得。

Link to this page