Pset_EvaporativeCoolerPHistory

BACnet MVD

#### 7.5.4.45 Pset_EvaporativeCoolerPHistory

PSET_PERFORMANCEDRIVEN / IfcEvaporativeCooler

Natural language names

| Evaporative Cooler PHistory

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

WaterSumpTemperature

P_REFERENCEVALUE / IfcTimeSeries / IfcThermodynamicTemperatureMeasure

| Water Sump Temperature | Water sump temperature.
| 液温度 | 液温度　（水溜り温度）

Effectiveness

P_REFERENCEVALUE / IfcTimeSeries / IfcRatioMeasure

| Effectiveness | Ratio of the change in dry bulb temperature of the (primary) air stream to the difference between the entering dry bulb temperature of the (primary) air and the wet-bulb temperature of the (secondary) air.
| 効率 | （一次）空気の入力乾球温度と（二次）空気の湿球温度の差に対する（一次）空気の流れの乾球温度の変化の割合。

SensibleHeatTransferRate

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Sensible Heat Transfer Rate | Sensible heat transfer rate to primary air flow.
| 顕熱交換量 | 一次空気流の顕熱交換量

LatentHeatTransferRate

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Latent Heat Transfer Rate | Latent heat transfer rate to primary air flow.
| 潜熱交換量 | 一次空気流の潜熱交換量

TotalHeatTransferRate

P_REFERENCEVALUE / IfcTimeSeries / IfcPowerMeasure

| Total Heat Transfer Rate | Total heat transfer rate to primary air flow.
| 全熱交換量 | 一次空気流の全熱交換量

Link to this page