Pset_DistributionChamberElementTypeMeterChamber

BACnet MVD

#### 6.2.4.7 Pset_DistributionChamberElementTypeMeterChamber

PSET_TYPEDRIVENOVERRIDE / IfcDistributionChamberElement / METERCHAMBER

Natural language names

| Distribution Chamber Element Type Meter Chamber

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ChamberLengthOrRadius

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Chamber Length Or Radius | Length or, in the event of the shape being circular in plan, the radius of the chamber.
| チャンバーの長さあるいは半径 | チャンバーの長さあるいは円形チャンバーの半径。

ChamberWidth

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Chamber Width | Width, in the event of the shape being non circular in plan.
| チャンバーの幅 | 非円形チャンバーの幅。

WallMaterial

P_REFERENCEVALUE / IfcMaterialDefinition

| Wall Material | The material from which the wall of the chamber is constructed. NOTE: It is assumed that chamber walls will be constructed of a single material.
| 壁の材質 | ダクトスペース壁の材質。 注：ダクトスペースの壁は単層と仮定する

WallThickness

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Wall Thickness | The thickness of the chamber wall construction . NOTE: It is assumed that chamber walls will be constructed at a single thickness.
| 壁厚さ | ダクトスペース壁の厚さ。 注：ダクトスペースの壁は単層と仮定する

BaseMaterial

P_REFERENCEVALUE / IfcMaterialDefinition

| Base Material | The material from which the base of the chamber is constructed. NOTE: It is assumed that chamber base will be constructed of a single material.
| 床の材質 | ダクトスペース床面の材質。 注：ダクトスペースの床は単層と仮定する

BaseThickness

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Base Thickness | The thickness of the chamber base construction. NOTE: It is assumed that chamber base will be constructed at a single thickness.
| 床の厚さ | ダクトスペース床面の厚さ。 注：ダクトスペースの床は単層と仮定する

AccessCoverMaterial

P_REFERENCEVALUE / IfcMaterialDefinition

| Access Cover Material | The material from which the access cover to the chamber is constructed. NOTE: It is assumed that chamber walls will be constructed of a single material.
| アクセス（点検）カバーの材質 | アクセス（点検）カバーの材質。 注：バイブスペースの壁は単層と仮定する

Link to this page