PEnum_ValveMechanism

BACnet MVD

#### 7.5.4.199 PEnum_ValveMechanism

Natural language names

Constants

Name | Description
--- | ---

BALL

| Ball | Valve that has a ported ball that can be turned relative to the body seat ports

BUTTERFLY

| Butterfly | Valve in which a streamlined disc pivots about a diametric axis

CONFIGUREDGATE

| Configured Gate | Screwdown valve in which the closing gate is shaped in a configured manner to have a more precise control of pressure and flow change across the valve

GLAND

| Gland | Valve with a tapered seating, in which a rotatable plug is retained by means of a gland and gland packing

GLOBE

| Globe | Screwdown valve that has a spherical body

LUBRICATEDPLUG

| Lubricated Plug | Plug valve in which a lubricant is injected under pressure between the plug face and the body

NEEDLE

| Needle | Valve for regulating the flow in or from a pipe, in which a slender cone moves along the axis of flow to close against a fixed conical seat

PARALLELSLIDE

| Parallel Slide | Screwdown valve that has a machined plate that slides in formed grooves to form a seal

PLUG

| Plug | Plug valve in which a lubricant is injected under pressure between the plug face and the body

WEDGEGATE

| Wedge Gate | Screwdown valve that has a wedge shaped plate fitting into tapered guides to form a seal

OTHER

| (other) | Value is not listed.

NOTKNOWN

| (unknown) | Value is unknown.

UNSET

| (unset) | Value has not been specified.

References: Pset_ValveTypeCommon

Link to this page