Pset_EnvironmentalImpactValues

BACnet MVD

#### 5.4.4.11 Pset_EnvironmentalImpactValues

PSET_TYPEDRIVENOVERRIDE / IfcElement

Natural language names

| Environmental Impact Values

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 1
Pset_EnvironmentalImpactValues |  |  |  |
LeadInTime |  |  | ADDED |
Duration |  |  | ADDED |
LeadOutTime |  |  | ADDED |

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

TotalPrimaryEnergyConsumption

P_SINGLEVALUE / IfcEnergyMeasure

| Total Primary Energy Consumption | Quantity of energy used as defined in ISO21930:2007.
| ConsommationTotaleEnergiePrimaire | Consommation d'énergie primaire utilisée, telle que définie dans les normes ISO21930:2007 [NDT : ou NF P01-010]
| 主なエネルギー消費の総量 | ISO21930:2007.で定義されているエネルギー量。

WaterConsumption

P_SINGLEVALUE / IfcVolumeMeasure

| Water Consumption | Quantity of water used.
| ConsommationEau | Quantité d'eau utilisée [NDT : telle que définie dans la norme NF P01-010]
| 水消費量 | 水の消費量。

HazardousWaste

P_SINGLEVALUE / IfcMassMeasure

| Hazardous Waste | Quantity of hazardous waste generated.
| DechetsDangereux | Quantité de déchets dangereux générés [NDT : tels que définis dans la norme NF P01-010]
| 有害廃棄物 | 生成される有害廃棄物の量。

NonHazardousWaste

P_SINGLEVALUE / IfcMassMeasure

| Non Hazardous Waste | Quantity of non hazardous waste generated.
| DechetsNonDangereux | Quantité de déchets non dangereux générés [NDT : tels que définis dans la norme NF P01-010]
| 一般廃棄物 | 生成される一般廃棄物の量。

ClimateChange

P_SINGLEVALUE / IfcMassMeasure

| Climate Change | Quantity of greenhouse gases emitted calculated in equivalent CO2.
| ChangementClimatique | Quantité d'émissions de gaz à effet de serre exprimée en Kg d'équivalent CO2, selon les normes PrEN15804:2008 [NDT : ou NF P01-010]
| 気候変化 | 算出されたCO2と等しい放出される温室効果ガスの量。

AtmosphericAcidification

P_SINGLEVALUE / IfcMassMeasure

| Atmospheric Acidification | Quantity of gases responsible for the atmospheric acidification calculated in equivalent SO2.
| AcidificationAtmospherique | Quantité de gaz responsables de l'acidification atmosphérique exprimée en Kg d'équivalent SO2, selon les normes PrEN15804:2008 [NDT : ou NF P01-010]
| 大気の酸性化 | 算出されたSO2と等しい大気中の酸性化の責任を負うガスの量。

RenewableEnergyConsumption

P_SINGLEVALUE / IfcEnergyMeasure

| Renewable Energy Consumption | Quantity of renewable energy used as defined in ISO21930:2007
| ConsommationEnergieRenouvelable | Consommation d'énergie renouvelable telle que définie dans les normes ISO21930:2007 [NDT : ou NF P01-010]
| 継続可能なエネルギー消費量 | ISO21930:2007 で定義されている継続可能なエネルギー消費量。

NonRenewableEnergyConsumption

P_SINGLEVALUE / IfcEnergyMeasure

| Non Renewable Energy Consumption | Quantity of non-renewable energy used as defined in ISO21930:2007
| ConsommationEnergieNonRenouvelable | Consommation d'énergie non renouvelable telle que définie dans les normes ISO21930:2007 [NDT : ou NF P01-010]
| 継続不可能なエネルギー消費量 | ISO21930:2007 で定義されている継続不可能なエネルギー消費量。

ResourceDepletion

P_SINGLEVALUE / IfcMassMeasure

| Resource Depletion | Quantity of resources used calculated in equivalent antimony.
| EpuisementRessources | Quantité de ressources consommées exprimée en équivalent Antimoine [NDT : selon la norme NF P01-010]
| 資源の枯渇 | 算出されたアンチモンと同等な資源の量。

InertWaste

P_SINGLEVALUE / IfcMassMeasure

| Inert Waste | Quantity of inert waste generated .
| DechetsInertes | Quantité de déchets inertes générés [NDT : selon la norme NF P01-010]
| 安定廃棄物 | 生成される安定廃棄物の量。

RadioactiveWaste

P_SINGLEVALUE / IfcMassMeasure

| Radioactive Waste | Quantity of radioactive waste generated.
| DechetsRadioactifs | Quantité de déchets radioactifs générés [NDT : selon la norme NF P01-010]
| 放射性廃棄物 | 生成される放射性廃棄物の量。

StratosphericOzoneLayerDestruction

P_SINGLEVALUE / IfcMassMeasure

| Stratospheric Ozone Layer Destruction | Quantity of gases destroying the stratospheric ozone layer calculated in equivalent CFC-R11.
| DestructionCoucheOzoneStartospherique | Quantité de gaz destructeurs de la couche d'ozone exprimée en équivalent CFC-R11 [NDT : selon la norme NF P01-010]
| 大気オゾン層破壊 | 算出された CFC-R11と等しい大気オゾン層を破壊するガスの量。

PhotochemicalOzoneFormation

P_SINGLEVALUE / IfcMassMeasure

| Photochemical Ozone Formation | Quantity of gases creating the photochemical ozone calculated in equivalent ethylene.
| FormationOzonePhotochimique | Quantité de gaz producteurs d'ozone photochimique exprimée en équivalent ethylène [NDT : selon la norme NF P01-010]
| 光化学オゾン生成 | 算出された エチレンと等しい光化学オゾン層を生成するガスの量。

Eutrophication

P_SINGLEVALUE / IfcMassMeasure

| Eutrophication | Quantity of eutrophicating compounds calculated in equivalent PO4.
| Eutrophisation | Quantité de composés responsables de l'eutrophisation exprimée en équivalent P04 [NDT : selon la norme PrEN15804:2008]
| 富栄養化 | 算出されたPO4と等しい富栄養化を混合する量。

LeadInTime

P_SINGLEVALUE / IfcDuration

| Lead In Time | Lead in time before start of process.

Duration

P_SINGLEVALUE / IfcDuration

| Duration | Duration of process.

LeadOutTime

P_SINGLEVALUE / IfcDuration

| Lead Out Time | Lead out time after end of process.

Link to this page