IfcGeometricProjectionEnum

BACnet MVD

#### IfcGeometricProjectionEnum

Natural language names

| Geometric Projection Enum

##### Semantic definitions at the type

Type definition

IfcGeometricProjectionEnum defines the various representation types that can be semantically distinguished. Often different levels of detail of the shape representation are controlled by the representation type.

> HISTORY New enumeration in IFC2x2.

Enumeration definition

Constant | Description
--- | ---
GRAPH_VIEW | Geometric display representation that shows an abstract, often 1D element representation, e.g. representing a wall by its axis line.
SKETCH_VIEW | Geometric display representation that shows an abstract, often 2D element representation, e.g. representing a wall by its two foot print edges, surpressing any inner layer representation.
MODEL_VIEW | Geometric display representation that shows a full 3D element representation, e.g. representing a wall by its volumetric body.
PLAN_VIEW | Geometric display representation that shows a full 2D element representation, the level of detail often depends on the target scale, e.g. representing a wall by its two foot print edges and the edges of all inner layers. The projection is shown in ground view as seen from above.
REFLECTED_PLAN_VIEW | Geometric display representation that shows a full 2D element representation, the level of detail often depends on the target scale, e.g. representing a wall by its two foot print edges and the edges of all inner layers. The projection is shown in ground view as seen from below.
SECTION_VIEW | Geometric display representation that shows a full 2D element representation, the level of detail often depends on the target scale, e.g. representing a wall by its two inner/outer edges and the edges of all inner layers, if the element is cut by the section line.
ELEVATION_VIEW | Geometric display representation that shows a full 2D element representation, the level of detail often depends on the target scale, e.g. representing a wall by its bounding edges if the element is within an elevation view.
USERDEFINED | A user defined specification is given by the value of the UserDefinedTargetView attribute.
NOTDEFINED | No specification given.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcGeometricProjectionEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="graph_view"/>
<xs:enumeration value="sketch_view"/>
<xs:enumeration value="model_view"/>
<xs:enumeration value="plan_view"/>
<xs:enumeration value="reflected_plan_view"/>
<xs:enumeration value="section_view"/>
<xs:enumeration value="elevation_view"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcGeometricProjectionEnum = ENUMERATION OF (
GRAPH_VIEW,
SKETCH_VIEW,
MODEL_VIEW,
PLAN_VIEW,
REFLECTED_PLAN_VIEW,
SECTION_VIEW,
ELEVATION_VIEW,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcGeometricRepresentationSubContext

Link to this page