Qto_PileBaseQuantities

BACnet MVD

#### 7.8.5.2 Qto_PileBaseQuantities

QTO_TYPEDRIVENOVERRIDE / IfcPile

Natural language names

| Pile Base Quantities

Quantities

QTO-XML

Name | Type | Description
--- | --- | ---

Length

Q_LENGTH

| Length | Total length of the pile not taking into account any cut-out's or other processing features.

CrossSectionArea

Q_AREA

| Cross Section Area | Total area of the cross section (or profile) of the pile.

OuterSurfaceArea

Q_AREA

| Outer Surface Area | Total area of the extruded surfaces of the pile (not taking into account the end cap areas), normally generated as perimeter * length.

GrossSurfaceArea

Q_AREA

| Gross Surface Area | Total area of the pile, normally generated as perimeter * length + 2 * cross section area. It is the sum of OuterSurfaceArea + (2 x CrossSectionArea) and shall only be given, if the OuterSurfaceArea and CrossSectionArea cannot be established separately.

GrossVolume

Q_VOLUME

| Gross Volume | Total gross volume of the pile, not taking into account possible processing features (cut-out's, etc.) or openings and recesses.

NetVolume

Q_VOLUME

| Net Volume | Total net volume of the pile, taking into account possible processing features (cut-out's, etc.) or openings and recesses.

GrossWeight

Q_WEIGHT

| Gross Weight | Total gross weight of the pile without add-on parts, not taking into account possible processing features (cut-out's, etc.) or openings and recesses.

NetWeight

Q_WEIGHT

| Net Weight | Total net weight of the pile without add-on parts, taking into account possible processing features (cut-out's, etc.) or openings and recesses.

Link to this page