Pset_DistributionPortTypePipe

BACnet MVD

#### 6.2.4.17 Pset_DistributionPortTypePipe

PSET_TYPEDRIVENOVERRIDE / IfcDistributionPort / PIPE

Natural language names

| Distribution Port Type Pipe

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 1
Pset_DistributionPortTypePipe |  |  | MODIFIED | Instantiation changed from IfcDistributionPort/CHEMICAL to IfcDistributionPort/PIPE.

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ConnectionType

P_ENUMERATEDVALUE / IfcLabel / PEnum_PipeEndStyleTreatment

| Connection Type | The end-style treatment of the pipe port: BRAZED: Brazed. COMPRESSION: Compression. FLANGED: Flanged. GROOVED: Grooved. OUTSIDESLEEVE: Outside Sleeve. SOLDERED: Soldered. SWEDGE: Swedge. THREADED: Threaded. WELDED: Welded. OTHER: Another type of end-style has been applied. NONE: No end-style has been applied. USERDEFINED: User-defined port connection type. NOTDEFINED: Undefined port connection type.
| 接続タイプ | 物理ポート接続： - Coaxial: 同軸コネクタ. - DSub: D-Subコネクタ. - Infrared:赤外線 - RJ: 登録済みジャック. - Radio: 無線 - USB: USB.

ConnectionSubType

P_SINGLEVALUE / IfcLabel

| Connection Sub Type | The physical port connection subtype that further qualifies the ConnectionType.
| 接続サブタイプ | 物理ポート接続のサブタイプ。接続タイプ以外の情報を設定する場合に使用。下記の値を設定： - DSub: DA15, DB25, DC37, DD50, DE9, DE15 - Radio: IEEE802.11g, IEEE802.11n - RJ: 4P4C, 6P2C, 8P8C - USB: A, B, MiniA, MiniB, MicroA, MicroB

NominalDiameter

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Nominal Diameter | The nominal diameter of the pipe connection.
| 呼び径 | 配管の呼び径。

InnerDiameter

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Inner Diameter | The actual inner diameter of the pipe.
| 内径 | 配管の実内径。

OuterDiameter

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Outer Diameter | The actual outer diameter of the pipe.
| 外径 | 配管の実外径。

Temperature

P_BOUNDEDVALUE / IfcThermodynamicTemperatureMeasure

| Temperature | Temperature of the fluid.
| 温度 | 流体の温度。

VolumetricFlowRate

P_BOUNDEDVALUE / IfcVolumetricFlowRateMeasure

| Volumetric Flow Rate | The volumetric flow rate of the fluid.
| 体積流量 | 流体の体積流量。

MassFlowRate

P_BOUNDEDVALUE / IfcMassFlowRateMeasure

| Mass Flow Rate | The mass flow rate of the fluid.
| 質量流量 | 流体の質量流量。

FlowCondition

P_BOUNDEDVALUE / IfcPositiveRatioMeasure

| Flow Condition | Defines the flow condition as a percentage of the cross-sectional area.
| 流動状態 | 断面の充満率で流動状態を定義する。

Velocity

P_BOUNDEDVALUE / IfcLinearVelocityMeasure

| Velocity | The velocity of the fluid.
| 速度 | 流体の速度。

Pressure

P_BOUNDEDVALUE / IfcPressureMeasure

| Pressure | The pressure of the fluid.
| 圧力 | 流体の圧力。

Link to this page