IfcSlippageConnectionCondition

BACnet MVD

#### IfcSlippageConnectionCondition

Natural language names

| Schlupf-Übergangsbedingung
| Slippage Connection Condition

##### Semantic definitions at the entity

Entity definition

Describes slippage in support conditions or connection conditions. Slippage means that a relative displacement may occur in a support or connection before support or connection reactions are awoken.

Applicability:

- Point supports and connections,
- curve supports and connections,
- surface supports and connections.

> HISTORY New entity in IFC2x2.

Attribute definitions

# | Attribute | Type | Cardinality | Description | B
--- | --- | --- | --- | --- | ---
2 | SlippageX | IfcLengthMeasure | ? | Slippage in x-direction of the coordinate system defined by the instance which uses this resource object. |  | X
3 | SlippageY | IfcLengthMeasure | ? | Slippage in y-direction of the coordinate system defined by the instance which uses this resource object. |  | X
4 | SlippageZ | IfcLengthMeasure | ? | Slippage in z-direction of the coordinate system defined by the instance which uses this resource object. |  | X

##### Inherited definitions from supertypes

Entity inheritance
Attribute inheritance

# | Attribute | Type | Cardinality | Description | B
--- | --- | --- | --- | --- | ---
IfcStructuralConnectionCondition
1 | Name | IfcLabel | ? | Optionally defines a name for this connection condition. |  | X
IfcSlippageConnectionCondition
2 | SlippageX | IfcLengthMeasure | ? | Slippage in x-direction of the coordinate system defined by the instance which uses this resource object. |  | X
3 | SlippageY | IfcLengthMeasure | ? | Slippage in y-direction of the coordinate system defined by the instance which uses this resource object. |  | X
4 | SlippageZ | IfcLengthMeasure | ? | Slippage in z-direction of the coordinate system defined by the instance which uses this resource object. |  | X

##### Formal representations

XML Specification
`<xs:element name="IfcSlippageConnectionCondition" type="ifc:IfcSlippageConnectionCondition" substitutionGroup="ifc:IfcStructuralConnectionCondition" nillable="true"/>
<xs:complexType name="IfcSlippageConnectionCondition">
<xs:complexContent>
<xs:extension base="ifc:IfcStructuralConnectionCondition">
<xs:attribute name="SlippageX" type="ifc:IfcLengthMeasure" use="optional"/>
<xs:attribute name="SlippageY" type="ifc:IfcLengthMeasure" use="optional"/>
<xs:attribute name="SlippageZ" type="ifc:IfcLengthMeasure" use="optional"/>
</xs:extension>
</xs:complexContent>
</xs:complexType>
`
EXPRESS Specification
`ENTITY IfcSlippageConnectionCondition
SUBTYPE OF (IfcStructuralConnectionCondition);
SlippageX : OPTIONAL IfcLengthMeasure;
SlippageY : OPTIONAL IfcLengthMeasure;
SlippageZ : OPTIONAL IfcLengthMeasure;
END_ENTITY;

EXPRESS-G diagram

`

Link to this page