IfcCableCarrierFittingTypeEnum

BACnet MVD

#### IfcCableCarrierFittingTypeEnum

Natural language names

| Cable Carrier Fitting Type Enum
| Enumération des types de raccord de chemin de cable

##### Semantic definitions at the type

Type definition

The IfcCableCarrierFittingTypeEnum defines the range of different types of cable carrier fitting that can be specified.

> HISTORY New type in IFC2x2.

Enumeration definition

Constant | Description
--- | ---
BEND | A fitting that changes the route of the cable carrier.
CROSS | A fitting at which two branches are taken from the main route of the cable carrier simultaneously.
REDUCER | A fitting that changes the physical size of the main route of the cable carrier.
TEE | A fitting at which a branch is taken from the main route of the cable carrier.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcCableCarrierFittingTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="bend"/>
<xs:enumeration value="cross"/>
<xs:enumeration value="reducer"/>
<xs:enumeration value="tee"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcCableCarrierFittingTypeEnum = ENUMERATION OF (
BEND,
CROSS,
REDUCER,
TEE,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcCableCarrierFitting IfcCableCarrierFittingType

Link to this page