IfcMotorConnectionTypeEnum

BACnet MVD

#### IfcMotorConnectionTypeEnum

Natural language names

| Motor Connection Type Enum
| Enumération des types de connection du moteur

##### Semantic definitions at the type

Type definition

The IfcMotorConnectionTypeEnum defines the range of different types of motor connection that can be specified.

> HISTORY New type in IFC2x.

Enumeration definition

Constant | Description
--- | ---
BELTDRIVE | An indirect connection made through the medium of a shaped, flexible continuous loop.
COUPLING | An indirect connection made through the medium of the viscosity of a fluid.
DIRECTDRIVE | A direct, physical connection made between the motor and the driven device.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcMotorConnectionTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="beltdrive"/>
<xs:enumeration value="coupling"/>
<xs:enumeration value="directdrive"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcMotorConnectionTypeEnum = ENUMERATION OF (
BELTDRIVE,
COUPLING,
DIRECTDRIVE,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcMotorConnection IfcMotorConnectionType

Link to this page