IfcUnitaryControlElementTypeEnum

BACnet MVD

#### IfcUnitaryControlElementTypeEnum

Natural language names

| Unitary Control Element Type Enum
| Enumération des types d'élément de contrôle unitaire

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcUnitaryControlElementTypeEnum |  |  | ADDED |

##### Semantic definitions at the type

Type definition

The IfcUnitaryControlElementTypeEnum defines the range of different types and/or functions of unitary control elements possible.

> HISTORY New enumeration in IFC4.

Enumeration definition

Constant | Description
--- | ---
ALARMPANEL | A control element at which alarms are annunciated.
CONTROLPANEL | A control element at which devices that control or monitor the operation of a site, building or part of a building are located
GASDETECTIONPANEL | A control element at which the detection of gas is annunciated.
INDICATORPANEL | A control element at which equipment operational status, condition, safety state or other required parameters are indicated.
MIMICPANEL | A control element at which information that is available elsewhere is repeated or 'mimicked'.
HUMIDISTAT | A control element that senses and regulates the humidity of a system or space so that the humidity is maintained near a desired setpoint.
THERMOSTAT | A control element that senses and regulates the temperature of an element, system or space so that the temperature is maintained near a desired setpoint.
WEATHERSTATION | A control element that senses multiple climate properties such as temperature, humidity, pressure, wind, and rain.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcUnitaryControlElementTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="alarmpanel"/>
<xs:enumeration value="controlpanel"/>
<xs:enumeration value="gasdetectionpanel"/>
<xs:enumeration value="indicatorpanel"/>
<xs:enumeration value="mimicpanel"/>
<xs:enumeration value="humidistat"/>
<xs:enumeration value="thermostat"/>
<xs:enumeration value="weatherstation"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcUnitaryControlElementTypeEnum = ENUMERATION OF (
ALARMPANEL,
CONTROLPANEL,
GASDETECTIONPANEL,
INDICATORPANEL,
MIMICPANEL,
HUMIDISTAT,
THERMOSTAT,
WEATHERSTATION,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcUnitaryControlElement IfcUnitaryControlElementType

Link to this page