IfcFireSuppressionTerminalTypeEnum

BACnet MVD

#### IfcFireSuppressionTerminalTypeEnum

Natural language names

| Fire Suppression Terminal Type Enum
| Enumération des types d'appareil terminal d'extinction d'incendie

##### Semantic definitions at the type

Type definition

The IfcFireSuppressionTerminalTypeEnum defines the range of different types of fire suppression terminal that can be specified.

> HISTORY New type in IFC2x2.

Enumeration definition

Constant | Description
--- | ---
BREECHINGINLET | Symmetrical pipe fitting that unites two or more inlets into a single pipe. A breeching inlet may be used on either a wet or dry riser. Used by fire services personnel for fast connection of fire appliance hose reels. May also be used for foam.
FIREHYDRANT | Device, fitted to a pipe, through which a temporary supply of water may be provided. May also be termed a stand pipe.
HOSEREEL | A supporting framework on which a hose may be wound.
SPRINKLER | Device for sprinkling water from a pipe under pressure over an area.
SPRINKLERDEFLECTOR | Device attached to a sprinkler to deflect the water flow into a spread pattern to cover the required area.
USERDEFINED | User-defined type
NOTDEFINED | Underined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcFireSuppressionTerminalTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="breechinginlet"/>
<xs:enumeration value="firehydrant"/>
<xs:enumeration value="hosereel"/>
<xs:enumeration value="sprinkler"/>
<xs:enumeration value="sprinklerdeflector"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcFireSuppressionTerminalTypeEnum = ENUMERATION OF (
BREECHINGINLET,
FIREHYDRANT,
HOSEREEL,
SPRINKLER,
SPRINKLERDEFLECTOR,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcFireSuppressionTerminal IfcFireSuppressionTerminalType

Link to this page