Wall standard case

BACnet MVD

### E.5.6 Wall standard case

Format | ASCII | Size
--- | --- | ---
XML | File | 5571
STEP | File | 2932

View
Design Transfer View

Entity
IfcWallStandardCase
IfcWallType
IfcExtrudedAreaSolid
IfcRectangleProfileDef
IfcMaterialLayerSetUsage

This example illustrates a standard-case wall with extruded solid geometry, based on a material layer set usage definition. Figure 411 shows the resulting shape.

> NOTE The extruded profile is defined by IfcRectangleProfileDef

Figure 411 — Standard case wall with material layer set.

> NOTE There is no color information within the file, the displayed color has been set by the target application as a default.

Link to this page