IfcElectricFlowStorageDeviceTypeEnum

BACnet MVD

#### IfcElectricFlowStorageDeviceTypeEnum

Natural language names

| Electric Flow Storage Device Type Enum

##### Semantic definitions at the type

Type definition

The IfcElectricFlowStorageDeviceTypeEnum defines different types of electrical flow storage devices.

> HISTORY New type in IFC2x2.

Enumeration definition

Constant | Description
--- | ---
BATTERY | A device for storing energy in chemical form so that it can be released as electrical energy.
CAPACITORBANK | A device that stores electrical energy when an external power supply is present using the electrical property of capacitance.
HARMONICFILTER | A device that constantly injects currents that precisely correspond to the harmonic components drawn by the load.
INDUCTORBANK |
UPS | A device that provides a time limited alternative source of power supply in the event of failure of the main supply.
USERDEFINED | User-defined type.
NOTDEFINED | Undefined type.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcElectricFlowStorageDeviceTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="battery"/>
<xs:enumeration value="capacitorbank"/>
<xs:enumeration value="harmonicfilter"/>
<xs:enumeration value="inductorbank"/>
<xs:enumeration value="ups"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcElectricFlowStorageDeviceTypeEnum = ENUMERATION OF (
BATTERY,
CAPACITORBANK,
HARMONICFILTER,
INDUCTORBANK,
UPS,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcElectricFlowStorageDevice IfcElectricFlowStorageDeviceType

Link to this page