Pset_ProtectiveDeviceTypeFuseDisconnector

BACnet MVD

#### 7.4.4.64 Pset_ProtectiveDeviceTypeFuseDisconnector

PSET_TYPEDRIVENOVERRIDE / IfcProtectiveDevice / FUSEDISCONNECTOR

Natural language names

| Protective Device Type Fuse Disconnector

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

FuseDisconnectorType

P_ENUMERATEDVALUE / IfcLabel / PEnum_FuseDisconnectorType

| Fuse Disconnector Type | A list of the available types of fuse disconnector from which that required may be selected where: EngineProtectionDevice: A fuse whose characteristic is specifically designed for the protection of a motor or generator. FuseSwitchDisconnector: A switch disconnector in which a fuse link or a fuse carrier with fuse link forms the moving contact, HRC: A standard fuse (High Rupturing Capacity) OverloadProtectionDevice: A device that disconnects the supply when the operating conditions in an electrically undamaged circuit causes an overcurrent, SemiconductorFuse: A fuse whose characteristic is specifically designed for the protection of sem-conductor devices. SwitchDisconnectorFuse: A switch disconnector in which one or more poles have a fuse in series in a composite unit.
| ヒューズ遮断機のタイプ | 自家用発電連携側：モータや発電機の保護のために設計されているヒューズ。 地絡保護装置：これでヒューズリンクまたはヒューズリンクヒューズキャリアは、可動接点を形成するスイッチ断路器、 HRC：標準ヒューズ（高連動破壊容量） 漏電保護装置：電気的に破損して回路の動作条件は、過電流が発生する電源を切断装置 欠相保護付：その特性を具体的にsemが芯デバイスの保護のために設計されているヒューズ。 複合ヒューズ保護装置：その内の1つまたは複数の極は、複合ユニットに直列にヒューズを持っているスイッチ断路器。

VoltageLevel

P_ENUMERATEDVALUE / IfcLabel / PEnum_VoltageLevels

| Voltage Level | The voltage levels for which the data of the instance is valid. More than one value may be selected in the enumeration.
| 電圧レベル | 電圧レベルを選択。

IC60269

P_SINGLEVALUE / IfcElectricCurrentMeasure

| IC60269 | The breaking capacity in [A] for fuses in accordance with the IEC 60269 series.
| IC60269 | IECの60269シリーズに応じたヒューズの遮断容量[A]。

PowerLoss

P_SINGLEVALUE / IfcPowerMeasure

| Power Loss | The power loss in [W] of the fuse when the nominal current is flowing through the fuse.
| 電力損失 | 定格電流がヒューズに流れる時の電力損失[W]。

Link to this page