Pset_PrecastSlab

BACnet MVD

#### 7.8.4.6 Pset_PrecastSlab

PSET_TYPEDRIVENOVERRIDE / IfcSlab

Natural language names

| Precast Slab

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

TypeDesignator

P_SINGLEVALUE / IfcLabel

| Type Designator | Type designator for the precast concrete slab, expressing mainly the component type. Possible values are “Hollow-core”, “Double-tee”, “Flat plank”, etc.

ToppingType

P_SINGLEVALUE / IfcLabel

| Topping Type | Defines if a topping is applied and what kind. Values are “Full topping”, “Perimeter Wash”, “None”

EdgeDistanceToFirstAxis

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Edge Distance To First Axis | The distance from the left (‘West’) edge of the slab (in the direction of span of the components) to the axis of the first component.

DistanceBetweenComponentAxes

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Distance Between Component Axes | The distance between the axes of the components, measured along the ‘South’ edge of the slab.

AngleToFirstAxis

P_SINGLEVALUE / IfcPlaneAngleMeasure

| Angle To First Axis | The angle of rotation of the axis of the first component relative to the ‘West’ edge of the slab.

AngleBetweenComponentAxes

P_SINGLEVALUE / IfcPlaneAngleMeasure

| Angle Between Component Axes | The angle between the axes of each pair of components.

NominalThickness

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Nominal Thickness | The nominal overall thickness of the slab.

NominalToppingThickness

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Nominal Topping Thickness | The nominal thickness of the topping.

Link to this page