IfcElectricCurrentMeasure

BACnet MVD

#### IfcElectricCurrentMeasure

Natural language names

| Electric Current Measure
| Mesure de courant électrique

##### Semantic definitions at the type

Type definition

The value for the movement of electrically charged particles.

Usually measured in Ampere (A).

Type: REAL

> NOTE Type adapted from electric_current_measure defined in ISO 10303-41.

> HISTORY New type in IFC1.5.1.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcElectricCurrentMeasure">
<xs:restriction base="xs:double"/>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcElectricCurrentMeasure = REAL;
END_TYPE;

EXPRESS-G diagram

`

References: IfcMeasureValue

Link to this page