IfcAxis2Placement3D

BACnet MVD

#### IfcAxis2Placement3D

Natural language names

| Einfügepunkt mit zwei Achsen - dreidimensionaler Raum (3D)
| Axis2 Placement3 D

##### Semantic definitions at the entity

Entity definition

The IfcAxis2Placement3D provides location and orientations to place items in a three-dimensional space. The attribute Axis defines the Z direction, RefDirection the X direction. The Y direction is derived.

> NOTE The RefDirection does not have to be orthogonal to Axis.

If the attribute values for Axis and RefDirection are not given, the placement defaults to P[1] (x-axis) as [1.,0.,0.], P[2] (y-axis) as [0.,1.,0.] and P[3] (z-axis) as [0.,0.,1.].

> Figure 313 illustrates the definition of the IfcAxis2Placement3D within the three-dimensional coordinate system.

Figure 313 — Axis2 placement 3D |

> NOTE Definition according to ISO/CD 10303-42:1992
> The location and orientation in three dimensional space of three mutually perpendicular axes. An axis2_placement_3D is defined in terms of a point (inherited from placement supertype) and two (ideally orthogonal) axes. It can be used to locate and orientate a non axi-symmetric object in space and to define a placement coordinate system. The entity includes a point which forms the origin of the placement coordinate system. Two direction vectors are required to complete the definition of the placement coordinate system. The axis is the placement Z axis direction and the ref_direction is an approximation to the placement X axis direction.

> NOTE Entity adapted from axis2_placement_3d defined in ISO10303-42.

> HISTORY New entity in IFC1.5.

Attribute definitions

# | Attribute | Type | Cardinality | Description | B
--- | --- | --- | --- | --- | ---
2 | Axis | IfcDirection | ? | The exact direction of the local Z Axis. | X | X
3 | RefDirection | IfcDirection | ? | The direction used to determine the direction of the local X Axis. If necessary an adjustment is made to maintain orthogonality to the Axis direction. If Axis and/or RefDirection is omitted, these directions are taken from the geometric coordinate system. | X | X
| P :=IfcBuildAxes(Axis, RefDirection) | IfcDirection | L[3:3] | The normalized directions of the placement X Axis (P[1]) and the placement Y Axis (P[2]) and the placement Z Axis (P[3]). | X | X

Formal Propositions

Rule | Description
--- | ---
LocationIs3D | The dimensionality of the placement location shall be 3.
AxisIs3D | The Axis when given should only reference a three-dimensional IfcDirection.
RefDirIs3D | The RefDirection when given should only reference a three-dimensional IfcDirection.
AxisToRefDirPosition | The Axis and RefDirection shall not be parallel or anti-parallel.
AxisAndRefDirProvision | Either both, Axis and RefDirection are not given and therefore defaulted, or both shall be given.

##### Inherited definitions from supertypes

Entity inheritance
Attribute inheritance

# | Attribute | Type | Cardinality | Description | B
--- | --- | --- | --- | --- | ---
IfcRepresentationItem

LayerAssignment

IfcPresentationLayerAssignment
@AssignedItems

S[0:1]

Assignment of the representation item to a single or multiple layer(s). The LayerAssignments can override a LayerAssignments of the IfcRepresentation it is used within the list of Items.

> IFC2x3 CHANGE The inverse attribute LayerAssignments has been added.

> IFC4 CHANGE The inverse attribute LayerAssignment has been restricted to max 1. Upward compatibility for file based exchange is guaranteed.

X

StyledByItem

IfcStyledItem
@Item

S[0:1]

Reference to the IfcStyledItem that provides presentation information to the representation, e.g. a curve style, including colour and thickness to a geometric curve.

> IFC2x3 CHANGE The inverse attribute StyledByItem has been added.

X

X

IfcGeometricRepresentationItem
IfcPlacement
1 | Location | IfcCartesianPoint |  | The geometric position of a reference point, such as the center of a circle, of the item to be located. | X | X
| Dim :=Location.Dim | IfcDimensionCount |  | The space dimensionality of this class, derived from the dimensionality of the location. | X | X
IfcAxis2Placement3D
2 | Axis | IfcDirection | ? | The exact direction of the local Z Axis. | X | X
3 | RefDirection | IfcDirection | ? | The direction used to determine the direction of the local X Axis. If necessary an adjustment is made to maintain orthogonality to the Axis direction. If Axis and/or RefDirection is omitted, these directions are taken from the geometric coordinate system. | X | X
| P :=IfcBuildAxes(Axis, RefDirection) | IfcDirection | L[3:3] | The normalized directions of the placement X Axis (P[1]) and the placement Y Axis (P[2]) and the placement Z Axis (P[3]). | X | X

##### Formal representations

XML Specification
`<xs:element name="IfcAxis2Placement3D" type="ifc:IfcAxis2Placement3D" substitutionGroup="ifc:IfcPlacement" nillable="true"/>
<xs:complexType name="IfcAxis2Placement3D">
<xs:complexContent>
<xs:extension base="ifc:IfcPlacement">
<xs:sequence>
<xs:element name="Axis" type="ifc:IfcDirection" nillable="true" minOccurs="0"/>
<xs:element name="RefDirection" type="ifc:IfcDirection" nillable="true" minOccurs="0"/>
</xs:sequence>
</xs:extension>
</xs:complexContent>
</xs:complexType>
`
EXPRESS Specification
`ENTITY IfcAxis2Placement3D
SUBTYPE OF (IfcPlacement);
Axis : OPTIONAL IfcDirection;
RefDirection : OPTIONAL IfcDirection;
DERIVE
P : LIST [3:3] OF IfcDirection := IfcBuildAxes(Axis, RefDirection);
WHERE
LocationIs3D : SELF\IfcPlacement.Location.Dim = 3;
AxisIs3D : (NOT (EXISTS (Axis))) OR (Axis.Dim = 3);
RefDirIs3D : (NOT (EXISTS (RefDirection))) OR (RefDirection.Dim = 3);
AxisToRefDirPosition : (NOT (EXISTS (Axis))) OR (NOT (EXISTS (RefDirection))) OR (IfcCrossProduct(Axis,RefDirection).Magnitude > 0.0);
AxisAndRefDirProvision : NOT ((EXISTS (Axis)) XOR (EXISTS (RefDirection)));
END_ENTITY;

EXPRESS-G diagram

`

References: IfcRelConnectsStructuralMember IfcStructuralAnalysisModel IfcStructuralPointConnection IfcCsgPrimitive3D IfcPolygonalBoundedHalfSpace IfcSectionedSpine IfcSweptAreaSolid IfcElementarySurface IfcSweptSurface IfcAxis2Placement IfcLightSourceGoniometric

Link to this page