Pset_StructuralSurfaceMemberVaryingThickness

BACnet MVD

#### 7.7.4.1 Pset_StructuralSurfaceMemberVaryingThickness

PSET_TYPEDRIVENOVERRIDE / IfcStructuralSurfaceMemberVarying

Natural language names

| Structural Surface Member Varying Thickness

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Thickness1

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Thickness1 | First thickness parameter of a surface member with varying thickness

Location1Local

P_LISTVALUE / IfcLengthMeasure

| Location1 Local | Local x,y coordinates of the point in which Thickness1 is given

Location1Global

P_LISTVALUE / IfcLengthMeasure

| Location1 Global | Global X,Y,Z coordinates of the point in which Thickness1 is given

Thickness2

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Thickness2 | Second thickness parameter of a surface member with varying thickness

Location2Local

P_LISTVALUE / IfcLengthMeasure

| Location2 Local | Local x,y coordinates of the point in which Thickness2 is given

Location2Global

P_LISTVALUE / IfcLengthMeasure

| Location2 Global | Global X,Y,Z coordinates of the point in which Thickness2 is given

Thickness3

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Thickness3 | Third thickness parameter of a surface member with varying thickness

Location3Local

P_LISTVALUE / IfcLengthMeasure

| Location3 Local | Local x,y coordinates of the point in which Thickness3 is given

Location3Global

P_LISTVALUE / IfcLengthMeasure

| Location3 Global | Global X,Y,Z coordinates of the point in which Thickness3 is given

Link to this page