Pset_SensorTypeSmokeSensor

BACnet MVD

#### 7.2.4.64 Pset_SensorTypeSmokeSensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / SMOKESENSOR

Natural language names

| Sensor Type Smoke Sensor

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

CoverageArea

P_SINGLEVALUE / IfcAreaMeasure

| Coverage Area | The floor area that is covered by the sensor (typically measured as a circle whose center is at the location of the sensor).
| 測定範囲 | センサでカバーされている床面積。(通常、センターがセンサの位置にある円として測定される)

SetPointConcentration

P_BOUNDEDVALUE / IfcPositiveRatioMeasure

| Set Point Concentration | The smoke concentration value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
| 煙濃度設定値 | 感知される煙濃度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。

HasBuiltInAlarm

P_SINGLEVALUE / IfcBoolean

| Has Built In Alarm | Indicates whether the smoke sensor is included as an element within a smoke alarm/sensor unit (TRUE) or not (FALSE).
| 煙警報器に含まれているか | 煙センサーが煙警報センサユニットの中に要素として含まれているか(TRUE)、否か(FALSE)を識別する。

Link to this page