Pset_TankOccurrence

BACnet MVD

#### 7.5.4.89 Pset_TankOccurrence

PSET_OCCURRENCEDRIVEN / IfcTank

Natural language names

| Tank Occurrence

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

TankComposition

P_ENUMERATEDVALUE / IfcLabel / PEnum_TankComposition

| Tank Composition | Defines the level of element composition where. COMPLEX: A set of elementary units aggregated together to fulfill the overall required purpose. ELEMENT: A single elementary unit that may exist of itself or as an aggregation of partial units.. PARTIAL: A partial elementary unit.
| 水槽構成 | 定義　構成要素のレベル　　　　　　　　　　　　　　　　　　　　　　　複合：A　全般的に要求された目的を達成するために集められた基本ユニットのセット　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　要素：A それ自身あるいは部分的ユニットの集まりとしてある単一基本ユニット　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　　部分的：A 部分的な基本単位

HasLadder

P_SINGLEVALUE / IfcBoolean

| Has Ladder | Indication of whether the tank is provided with a ladder (set TRUE) for access to the top. If no ladder is provided then value is set FALSE. Note: No indication is given of the type of ladder (gooseneck etc.)
| 梯子有り | 上部を点検するための梯子(TRUEに設定）をタンクに備えているかどうかの表示　もし、梯子が備え付けられていなければ値はFALSEと設定される。　　注：表示がない場合は梯子のタイプが与えられる（グースネック他）

HasVisualIndicator

P_SINGLEVALUE / IfcBoolean

| Has Visual Indicator | Indication of whether the tank is provided with a visual indicator (set TRUE) that shows the water level in the tank. If no visual indicator is provided then value is set FALSE.
| 目視型表示器有り | タンクの水位を示す目視型表示器（TRUEに設定)が備えつけられているかどうかの表示。もし目視型表示器が備えつけられていなければ、値はFALSEと設定される。

Link to this page