Pset_SensorTypeHeatSensor

BACnet MVD

#### 7.2.4.52 Pset_SensorTypeHeatSensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / HEATSENSOR

Natural language names

| Sensor Type Heat Sensor

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

CoverageArea

P_SINGLEVALUE / IfcAreaMeasure

| Coverage Area | The area that is covered by the sensor (typically measured as a circle whose center is at the location of the sensor).
| 測定範囲 | センサでカバーされている範囲。(通常、センターがセンサの位置にある円として測定される)

SetPointTemperature

P_BOUNDEDVALUE / IfcThermodynamicTemperatureMeasure

| Set Point Temperature | The temperature value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
| 温度設定値 | 感知される温度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。

RateOfTemperatureRise

P_SINGLEVALUE / IfcTemperatureRateOfChangeMeasure

| Rate Of Temperature Rise | The rate of temperature rise that is to be sensed as being hazardous.
| 温度上昇率 | 危険であるとして感じられることになっている温度上昇率。

Link to this page