Pset_CooledBeamTypeCommon

BACnet MVD

#### 7.5.4.26 Pset_CooledBeamTypeCommon

PSET_TYPEDRIVENOVERRIDE / IfcCooledBeam

Natural language names

| Cooled Beam Type Common

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC4 Addendum 2
Pset_CooledBeamTypeCommon |  |  |  |
PipeConnection |  |  | ADDED |
PipeConnectionEnum |  |  | DELETED |

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

Reference

P_SINGLEVALUE / IfcIdentifier *

| Bauteiltyp | Bezeichnung zur Zusammenfassung gleichartiger Bauteile zu einem Bauteiltyp (auch Konstruktionstyp genannt). Alternativ zum Namen des "Typobjekts", insbesondere wenn die Software keine Typen unterstützt.
| Reference | Reference ID for this specified type in this project (e.g. type 'A-1'), Also referred to as "construction type". It should be provided as an alternative to the name of the "object type", if the software does not support object types.
| Reference | Référence à l'identifiant d'un type spécifié dans le contexte du projet (exemple : "type A1") pour désigner un "type de construction". Une alternative au nom d'un objet type lorsque les objets types ne sont pas gérés par le logiciel.
| 参照記号 | このプロジェクトにおける参照記号(例：A-1)。分類コードではなく内部で使用されるプロジェクトタイプとして使用されるもの。
| 参考号 | 若未采用已知的分类系统，则该属性为该项目中该类型构件的参考编号（例如，类型A-1）。

Status

P_ENUMERATEDVALUE / IfcLabel / PEnum_ElementStatus*

| Status | Status bzw. Phase des Bauteils insbesondere beim Bauen im Bestand. "Neu" (new) neues Bauteil als Ergänzung, "Bestand" (existing) bestehendes Bauteil, dass erhalten bleibt, "Abbruch" (demolish) Bauteil, das abgebrochen wird, "Temporär" (temporary) Bauteil und andere Bauelemente, die vorübergehend eingebaut werden (wie Abstützungen, etc.)
| Status | Status of the element, predominately used in renovation or retrofitting projects. The status can be assigned to as "New" - element designed as new addition, "Existing" - element exists and remains, "Demolish" - element existed but is to be demolished, "Temporary" - element will exists only temporary (like a temporary support structure).
| Statut | Statut de l'élément, principalement utilisé dans les projets de rénovation et de réhabilitation. Le statut a pour valeur NOUVEAU pour un nouvel élément, EXISTANT pour un élément existant qui est conservé, DEMOLI pour un élément existant à démolir et TEMPORAIRE pour un élément temporaire (comme une structure support provisoire).
| 状態 | 要素（主にリノベーションまたは改修プロジェクトにおいて）の状態。 状態は、「新規(New)」－新しく追加される要素。「既存」－要素は存在し、かつ残りもの。「破壊」－要素は存在したが、廃棄されるもの。「一時的」－一時的に存在する要素（一時的にサポートしている構造のようなもの）。

IsFreeHanging

P_SINGLEVALUE / IfcBoolean

| Is Free Hanging | Is it free hanging type (not mounted in a false ceiling)?

PipeConnection

P_ENUMERATEDVALUE / IfcLabel / PEnum_CooledBeamPipeConnection

| Pipe Connection Enum | The manner in which the pipe connection is made to the cooled beam.

WaterFlowControlSystemType

P_ENUMERATEDVALUE / IfcLabel / PEnum_CooledBeamWaterFlowControlSystemType

| Water Flow Control System Type | Factory fitted waterflow control system.

WaterPressureRange

P_BOUNDEDVALUE / IfcPressureMeasure

| Water Pressure Range | Allowable water circuit working pressure range.

NominalCoolingCapacity

P_SINGLEVALUE / IfcPowerMeasure

| Nominal Cooling Capacity | Nominal cooling capacity.

NominalSurroundingTemperatureCooling

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Nominal Surrounding Temperature Cooling | Nominal surrounding temperature (refers to nominal cooling capacity).

NominalSurroundingHumidityCooling

P_SINGLEVALUE / IfcNormalisedRatioMeasure

| Nominal Surrounding Humidity Cooling | Nominal surrounding humidity (refers to nominal cooling capacity).

NominalSupplyWaterTemperatureCooling

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Nominal Supply Water Temperature Cooling | Nominal supply water temperature (refers to nominal cooling capacity).

NominalReturnWaterTemperatureCooling

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Nominal Return Water Temperature Cooling | Nominal return water temperature (refers to nominal cooling capacity).

NominalWaterFlowCooling

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Nominal Water Flow Cooling | Nominal water flow (refers to nominal cooling capacity).

NominalHeatingCapacity

P_SINGLEVALUE / IfcPowerMeasure

| Nominal Heating Capacity | Nominal heating capacity.

NominalSurroundingTemperatureHeating

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Nominal Surrounding Temperature Heating | Nominal surrounding temperature (refers to nominal heating capacity).

NominalSupplyWaterTemperatureHeating

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Nominal Supply Water Temperature Heating | Nominal supply water temperature (refers to nominal heating capacity).

NominalReturnWaterTemperatureHeating

P_SINGLEVALUE / IfcThermodynamicTemperatureMeasure

| Nominal Return Water Temperature Heating | Nominal return water temperature (refers to nominal heating capacity).

NominalWaterFlowHeating

P_SINGLEVALUE / IfcVolumetricFlowRateMeasure

| Nominal Water Flow Heating | Nominal water flow (refers to nominal heating capacity).

IntegratedLightingType

P_ENUMERATEDVALUE / IfcLabel / PEnum_CooledBeamIntegratedLightingType

| Integrated Lighting Type | Integrated lighting in cooled beam.

FinishColor

P_SINGLEVALUE / IfcLabel

| Finish Color | Finish color for cooled beam.

CoilLength

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Coil Length | Length of coil.

CoilWidth

P_SINGLEVALUE / IfcPositiveLengthMeasure

| Coil Width | Width of coil.

Link to this page