IfcFlowMeterTypeEnum

BACnet MVD

#### IfcFlowMeterTypeEnum

Natural language names

| Flow Meter Type Enum
| Enumération des types d'appareil de mesure de débit

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcFlowMeterTypeEnum |  |  |  |
ELECTRICMETER | X | X | DELETED |
FLOWMETER | X | X | DELETED |

##### Semantic definitions at the type

Type definition

This enumeration defines various types of flow meter:

> HISTORY New enumeration in IFC2x2.

> IFC4 CHANGE ELECTRICMETER and FLOWMETER removed.

Enumeration definition

Constant | Description
--- | ---
ENERGYMETER | An electric meter or energy meter is a device that measures the amount of electrical energy supplied to or produced by a residence, business or machine.
GASMETER | A device that measures the quantity of a gas or fuel.
OILMETER | A device that measures the quantity of oil.
WATERMETER | A device that measures the quantity of water.
USERDEFINED | User-defined meter type
NOTDEFINED | Undefined meter type

##### Formal representations

XML Specification
`<xs:simpleType name="IfcFlowMeterTypeEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="energymeter"/>
<xs:enumeration value="gasmeter"/>
<xs:enumeration value="oilmeter"/>
<xs:enumeration value="watermeter"/>
<xs:enumeration value="userdefined"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcFlowMeterTypeEnum = ENUMERATION OF (
ENERGYMETER,
GASMETER,
OILMETER,
WATERMETER,
USERDEFINED,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcFlowMeter IfcFlowMeterType

Link to this page