Pset_MaterialWater

BACnet MVD

#### 8.10.5.11 Pset_MaterialWater

PSET_TYPEDRIVENOVERRIDE / IfcMaterial

Natural language names

| Material Water

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

IsPotable

P_SINGLEVALUE / IfcBoolean

| Is Potable | If TRUE, then the water is considered potable.

Hardness

P_SINGLEVALUE / IfcIonConcentrationMeasure

| Hardness | Water hardness as positive, multivalent ion concentration in the water (usually concentrations of calcium and magnesium ions in terms of calcium carbonate).

AlkalinityConcentration

P_SINGLEVALUE / IfcIonConcentrationMeasure

| Alkalinity Concentration | Maximum alkalinity concentration (maximum sum of concentrations of each of the negative ions substances measured as CaCO3).

AcidityConcentration

P_SINGLEVALUE / IfcIonConcentrationMeasure

| Acidity Concentration | Maximum CaCO3 equivalent that would neutralize the acid.

ImpuritiesContent

P_SINGLEVALUE / IfcNormalisedRatioMeasure

| Impurities Content | Fraction of impurities such as dust to the total amount of water. This is measured in weight of impurities per weight of water and is therefore unitless.

DissolvedSolidsContent

P_SINGLEVALUE / IfcNormalisedRatioMeasure

| Dissolved Solids Content | Fraction of the dissolved solids to the total amount of water. This is measured in weight of dissolved solids per weight of water and is therefore unitless.

PHLevel

P_SINGLEVALUE / IfcPHMeasure

| PHLevel | Maximum water PH in a range from 0-14.

Link to this page