Pset_ProjectOrderMaintenanceWorkOrder

BACnet MVD

#### 6.5.4.5 Pset_ProjectOrderMaintenanceWorkOrder

PSET_TYPEDRIVENOVERRIDE / IfcProjectOrder / MAINTENANCEWORKORDER

Natural language names

| Project Order Maintenance Work Order

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

ProductDescription

P_SINGLEVALUE / IfcText

| Product Description | A textual description of the products that require the work.

WorkTypeRequested

P_SINGLEVALUE / IfcText

| Work Type Requested | Work type requested in circumstances where there are categorizations of types of work task. It could be used to identify a remedial task, minor work task, electrical task etc.

ContractualType

P_SINGLEVALUE / IfcText

| Contractual Type | The contractual type of the work.

IfNotAccomplished

P_SINGLEVALUE / IfcText

| If Not Accomplished | Comments if the job is not accomplished.

MaintenaceType

P_ENUMERATEDVALUE / IfcLabel / PEnum_MaintenanceType

| Maintenace Type | Identifies the predefined types of maintenance that can be done from which the type that generates the maintenance work order may be set where: ConditionBased: generated as a result of the condition of an asset or artefact being less than a determined value. Corrective: generated as a result of an immediate and urgent need for maintenance action. PlannedCorrective: generated as a result of immediate corrective action being needed but with sufficient time available for the work order to be included in maintenance planning. Scheduled: generated as a result of a fixed, periodic maintenance requirement.

FaultPriorityType

P_ENUMERATEDVALUE / IfcLabel / PEnum_PriorityType

| Fault Priority Type | Identifies the predefined types of priority that can be assigned from which the type may be set where: High: action is required urgently. Medium: action can occur within a reasonable period of time. Low: action can occur when convenient.

LocationPriorityType

P_ENUMERATEDVALUE / IfcLabel / PEnum_PriorityType

| Location Priority Type | Identifies the predefined types of priority that can be assigned from which the type may be set where: High: action is required urgently. Medium: action can occur within a reasonable period of time. Low: action can occur when convenient.

ScheduledFrequency

P_SINGLEVALUE / IfcTimeMeasure

| Scheduled Frequency | The period of time between expected instantiations of a work order that may have been predefined.

Link to this page