Slab standard case

BACnet MVD

### E.5.5 Slab standard case

Format | ASCII | Size
--- | --- | ---
XML | File | 5396
STEP | File | 2740

View
Design Transfer View

Entity
IfcSlabStandardCase
IfcSlabType
IfcMaterialLayerSetUsage
IfcExtrudedAreaSolid
IfcIndexedPolyCurve

This example illustrates a standard-case slab with extruded solid geometry, based on a material layer set usage definition. Figure 410 shows the resulting shape.

> NOTE The extruded profile is defined by IfcIndexedPolyCurve

Figure 410 — Standard case slab with material layer set.

> NOTE There is no color information within the file, the displayed color has been set by the target application as a default.

Link to this page