IfcDoorPanelPositionEnum

BACnet MVD

#### IfcDoorPanelPositionEnum

Natural language names

| Door Panel Position Enum
| Énumération de la position du panneau de porte

Change log

Item | SPF | XML | Change | Description
--- | --- | --- | --- | ---
IFC2x3 to IFC4
IfcDoorPanelPositionEnum |  |  | MOVED | Schema changed from IFCSHAREDBLDGELEMENTS to IFCARCHITECTUREDOMAIN.

##### Semantic definitions at the type

Type definition

This enumeration defines the basic ways to describe the location of a door panel within a door lining.

> HISTORY New Enumeration in IFC2x

Figure 249 shows the designation of a door panel with PanelPosition = LEFT and a door panel with PanelPosition = RIGHT within a door style with OperationType = DOUBLE_DOOR_SINGLE_SWING. The position is given as shown in the XZ plane of the local placement, looking into the direction of the positive Y axis.

Figure 249 — Door panel positions

Enumeration definition

Constant | Description
--- | ---
LEFT |
MIDDLE |
RIGHT |
NOTDEFINED |

##### Formal representations

XML Specification
`<xs:simpleType name="IfcDoorPanelPositionEnum">
<xs:restriction base="xs:string">
<xs:enumeration value="left"/>
<xs:enumeration value="middle"/>
<xs:enumeration value="right"/>
<xs:enumeration value="notdefined"/>
</xs:restriction>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcDoorPanelPositionEnum = ENUMERATION OF (
LEFT,
MIDDLE,
RIGHT,
NOTDEFINED);
END_TYPE;

EXPRESS-G diagram

`

References: IfcDoorPanelProperties

Link to this page