IfcLuminousIntensityMeasure

BACnet MVD

#### IfcLuminousIntensityMeasure

Natural language names

| Luminous Intensity Measure
| Mesure de l'intensité lumineuse

##### Semantic definitions at the type

Type definition

An IfcLuminousIntensityMeasure is the value for the brightness of a body.

Usually measured in candela (cd).

Type: REAL

> NOTE Type adapted from luminous_intensity_measure defined in ISO 10303-41.

> HISTORY New type in IFC1.5.1.

##### Formal representations

XML Specification
`<xs:simpleType name="IfcLuminousIntensityMeasure">
<xs:restriction base="xs:double"/>
</xs:simpleType>
`
EXPRESS Specification
`TYPE IfcLuminousIntensityMeasure = REAL;
END_TYPE;

EXPRESS-G diagram

`

References: IfcMeasureValue

Link to this page