Pset_SensorTypeGasSensor

BACnet MVD

#### 7.2.4.51 Pset_SensorTypeGasSensor

PSET_TYPEDRIVENOVERRIDE / IfcSensor / GASSENSOR

Natural language names

| Sensor Type Gas Sensor

Properties

buildingSMART Data Dictionary

PSD-XML

Name | Type | Description
--- | --- | ---

GasDetected

P_SINGLEVALUE / IfcLabel

| Gas Detected | Identification of the gas that is being detected, according to chemical formula. For example, carbon monoxide is 'CO', carbon dioxide is 'CO2', oxygen is 'O2'.
| 対象ガス | 検出されているガスの識別。

SetPointConcentration

P_BOUNDEDVALUE / IfcPositiveRatioMeasure

| Set Point Concentration | The gas concentration value to be sensed. Use IfcPropertyBoundedValue.SetPointValue to set the set point value.
| ガス濃度設定値 | 感知されるガス濃度。 セットポイント値を置くために、IfcPropertyBoundedValue.SetPointValueを使用する。

CoverageArea

P_SINGLEVALUE / IfcAreaMeasure

| Coverage Area | The floor area that is covered by the sensor (typically measured as a circle whose center is at the location of the sensor).
| 測定範囲 | センサでカバーされている床面積。(通常、センターがセンサの位置にある円として測定される)

Link to this page